**Private Market**

**Acoustichoc®**

**TYPE DESCRIPTION FOR SHOCK RESISTANT SUSPENDED ACOUSTIC CEILING SPECIFICATIONS**

The suspended ceiling shall be made with Eurocoustic ACOUSTICHOC® type self supporting rock wool panels, clad on the exposed face with a veil complex reinforced with an armoured glass grill in colour: \***Available colours** and a natural glass fibre veil on the rear.

Modular dimensions shall be: **\*Available dimensions**

**Sound absorption** performance of the ACOUSTICHOC® panels shall be: **w = 1.00, Class A.**

 The installed ceiling’s **reaction to fire** shall be in accordance with: ***\**Available Euroclass**

The installed ceiling shall have the reaction to fire classification: **\*Available fire resistance**

The ceiling shall be installed on a **Quick-Lock** **grid**: **\*Available dimensions**made-up of galvanized steel profiles with visible base plate in white or colour.

A rim angle with the same colour shall ensure the peripheral finish to the right of walls and partitions.

Recommendations for installation:

* The installation shall be in accordance with the requirements of the standard NFP 68 203 1 and 2 DTU 58.1 and other DTU in force according to the type of premises.
* It is recommended to integrate the grills in the ceiling to balance the pressures and temperatures on either side of the ceiling.

**\* Insert your selection in the colour drop-down list**

