**Acoustished®**

**TYPE DESCRIPTION FOR EUROCOUSTIC CEILING SPECIFICATIONS**

The ceiling shall be Eurocoustic ACOUSTISHED® type. The rock wool ACOUSTISHED® panels shall be clad with a **decorative veil** **\*Decoration** on the exposed face. The rear of the panel shall be clad with a natural glass fibre veil.

For i**nstallation in suspended ceiling**, **module dimension** shall be **1500 x 1000 mm**.

Or

For **installation between supports, the actual dimensions** shall be **\*Dimensions**

**Thickness** of ACOUSTISHED® panels shall be **\*Thickness**

The panels shall be installed on a grid made with galvanised steel profiles whose visible base plate in white or coloured is 35 mm.

A rim angle with the same finish shall constitute the peripheral link.

The **sound absorption** performances of Eurocoustic ACOUSTISHED® panels shall be:

* **38 mm thickness: \*Thickness**
* **77 mm thickness: \*Thickness**

The installed panel’s **reaction to fire** shall be in accordance with **Euroclass** **\*Euroclass**

The **ceilings** shall be **perfectly 100% flat** whatever be the moisture content.

Recommendations for installation:

* Installation shall be in accordance with the requirements of the standard NFP 68 203 1 and 2; DTU 58.1 and other DTU in force according to the type of premises.
* It is recommended to integrate the grills in the ceiling to balance the pressures and temperatures on either side of the ceiling.

**\* Insert your selection in the colour drop-down list**

