**Area ®**

**TYPE DESCRIPTION FOR EUROCOUSTIC CEILING SPECIFICATIONS**

The suspended ceiling shall be made with Eurocoustic AREA type, rock wool, self-supporting panels provided with **Boreal finish**: satin white exposed face; natural glass fibre veil on the rear, edges closed with white paint.

**Modular dimensions** shall be **\*Dimensions**.

The ceiling shall be installed on a **grid** **\*Grid** made-up of galvanised steel profiles with visible base plate in white or colour.

A rim angle with the same colour shall ensure peripheral finish to the right of walls and partitions.

The installed ceiling shall be in accordance with **Euroclass A1**.

The **sound absorption** performances of the AREA® panels shall be:

* **w = 0.90, Class A**.

The installed AREA®panels shall not contain any **element favourable for the growth of micro-organisms**.

The **ceilings** shall be **perfectly 100% flat** whatever be the moisture content.

It shall be **cleanable with damp sponge** using a slightly alkaline detergent (PH<10).

Its **light reflection** co-efficient **shall be 88%.**

Recommendations for installation:

* Installation shall be in accordance with the requirements of the standard NFP 68 203 1 and 2; DTU 58.1 and other DTU in force according to the type of premises.
* It is recommended to integrate the grills in the ceiling to balance the pressures and temperatures on either side of the ceiling.

**\* Insert your selection in the colour drop-down list**

