**Minerval A®**

**TYPE DESCRIPTION FOR WHITE SUSPENDED CEILING SPECIFICATIONS**

The ceiling shall be made with Eurocoustic MINERVAL® type, rock wool, self-supporting panels, provided on the exposed face with a white veil and a natural glass fibre veil on the rear, the borders are straight.

**Modular dimensions**:

* **Available dimensions**

The **sound absorption** performances of the Minerval® panels shall be:

* **w = 0.90 for 12mm**
* **w = 0.95 for 15mm**

The installed ceiling shall be in accordance with **Euroclass A1**.

The **ceilings** shall be **perfectly 100% flat** whatever be the moisture content.

The ceiling shall be installed on a **Quick-Lock® grid**:

* **Available grids**

made with galvanized steel profiles with visible base plate in white.

A rim angle with the same colour shall ensure peripheral finish to the right of walls and partitions.

Assembly shall be in accordance with the reference report.

Recommendations for installation:

* Installation shall be in accordance with the requirements of the standard NFP 68 203 1 and 2; DTU 58.1 and other DTU in force according to the type of premises.
* It is recommended to integrate the grills in the ceiling to balance the pressures and temperatures on either side of the ceiling.

**\* Insert your selection in the colour drop-down list**

****